HOME SCIENCE PAPER 2
MARKING SCHEME          

	
	
	
Score
	
Actual score

	
1
	
PRESENTATION

a) Work well presented (1) and well folded (½)
b) Label (½) firmly stitched (1) on single fabric (½) without concealing details (½)
c) Pins/needles (½) and unnecessary tacking threads (½) and loose threads (½) removed
d) Make up the right half
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2
	
CUTTING OUT
a) All 5 pieces cut out (5x½)
b) Smooth cutting of skirt CF
c) CF cut on straight grain to within 3 mm
d) Smooth cutting of yoke CF
e) CF yoke cut on straight grain to within 3 mm
f) Smooth cutting of skirt CB
g) CB cut on straight grain to within 3mm
h) Smooth cutting of the pocket pieces
i) Smooth cutting of the skirt at waist back (1) front (1)  
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3
	
BACK DART
a) Made with straight stitchery (1) tapering to a point (½)
b) Thread ends well fastened at the point
c) Correct length of dart (9 cm) to within 5 mm
d) Correct width of dart (1.2 cm) to within 2 mm
e) Flatness of dart on WS (½) and RS (½) 
f) Dart pressed towards C.B 
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4
	
YOKE ATTACHMENT

a) Gathers evenly distributed
b) Gathers confined between the two dots
c) Seam made with stitchery (1) close to the fold (1)
             * (if not an overlaid seam give zero from c – g)
d) Correctly made seam i.e. yoke folded over the skirt
e) Raw edges well neatened (accept any correct method of neatening except pinking)
f) Evenness of the neatened seam allowance
g) Correct width of seam allowance 1 cm to within 2 mm
h) Yoke CF flash with skirt CF to within 2 mm
i) Correct shape () and size () to within 5 mm (superimpose)
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5
	
POCKET

a) Pocket pieces attached with straight stitchery (1x2)
b) Notches matching (1x2) if trimmed give zero (0)
c) Pocket pieces appropriately placed
d) Pocket pieces attached 5mm away from the side seams, to within 2 mm
e) Smooth stitchery round the pocket bag (2) and loop stitching half the pocket bag (1)
f) Correct shape (1) and size (1) of the pocket (superimpose)
g) Pocket mouth reinforced at the base (½) and top (½) to lie on the front piece (½)
h) Correct width of the mouth i.e. between the dots
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	6
	
SIDE SEAM – OPEN SEAM

a) Seam joined with straight stitchery above (1) and below (1) the pocket
b) Pocket mouth left unstitched
c) Raw edges well neatened below (1 x 2) & above (½ x 2) the pocket 
d) Evenness of the seam allowances below (1) and above (1) the pocket
e) Correct size of neatened seam allowances i.e. 1 cm to within 2 mm below (1) and above (1) the pocket
f) Back seam allowance snipped (½ x 2) and neatened above (½) and below (½) the pocket
g) Seam pressed open (1) and flat (1) at the hem
h) Back and front skirt pieces flash at waist 
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7
	
HEM

a) Raw edges concealed
b) Evenness of the hem depth (2) and correct size 3.3 cm to within 5 mm (2)
c) Flatness of the hem
d) Quality of slip hemming
e) Stitches evenly distributed
f) Correct tension
g) Stitches inconspicuous on the R.S
              ( if not slip-hemmed give zero (0) )
h) Side seam matching to within 2 mm at the hem
i) Hem flash at CF (1) and CB (1)
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	90
	

	
	TOTAL = (90÷ 2)  
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